# Annex 1: Technical Specification/Technical Offer form

Bidders must fill the section marked as ‘specifications offered’

**All the items should be guaranteed for at least a year**;

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Item** | **Specification** | **QTY** | **Offered Items**  |
| **1.** | Chemistry analyser Auto | 1.Bench top Auto- Chemistry Analiysr , Open reagent system .Equipment type Fully automatic discrete, STAT priority2.Analysis rate Constant speed 200T/H at least (without ISE)3.Test principle Colorimetry, turbidimetry4.Analysis method End-point, 2 kinetics, fixed-time, etc. support single/double wavelength, linear and non-linear calibration | 2 |  |
| **2.** | CBC Auto(Blood analyser) | Auto,large colour LCD display, 19 parameter+3 histograms WBC, Lymph#, Mid#, Gran#, Lymph%, Mid%, Gran%, RBC, HGB, HCT, MCV, MCH, MCHC, RDW-CV, RDW-SD, PLT, MPV, PDW, PCT and Histograms for WBC, RBC, PLT . Fully automatic calibration. Built in printer Power supply 220 50/60Hz. To be supplied with Accessory kit and Standard reagents for installation. | 1 |  |
| **3.** | Dental Chair | 1-Power Supply: 220V-50Hz2-The unit is equipped with a breaker and regulator for the water pressure on the main entrance3-The filling of the patient's cup and washing the spit is controlled from two different places (doctor's table and auxiliary nurse table)4-The unit is equipped with an indicator to read the air pressure on the grips installed on the tray5-The tool holder and fists are of stainless quality and easy to clean and are equipped with additional stainless steel tool plate6-Cold halogen light center7-The light is equipped with a glass reflector, heat protection 8-The umit is equipped with a water heater. | 2 |  |
| **4.** | Lensometer | 1- Power supply : AC 220 Volt / 50 Hz .2-Digital system.3-The bidder should specify Lens diameter.4-LCD screen and its specifications should be specified by the bidder.5-Lens marker 6-Built-in thermal printer .7-Pupil Distance measurement is preferred . | 1 |  |
| **5.** | ECG machine | Electrocardiogram Machine (ECG) 3 channels at least, Portable, operating on AC and with internal rechergeable lithium batteries. Portable, built in thermal printer, recheargeable battery, AC/DC power. Automatic ECG measurement and interpretation,  the bidder should be mention the all specfications.With Thermal paper role qty.30 | 1 |  |
| **6.** | Bronchscope  | The specification of the scope: High resolution image quality.1-Slimmer outer diameter: 4.8mm at least2-Helps support inspection to bronchi, while maintaining a 2.0 mm at least instrument channel for a diverse of purposes.3-Depth of field 3-50 mm at least4-Field of view 120◦5-Working length 600mm at least6-Included video processor with built in LED light source with HDTV image and monitor  | 1 |  |
| **7.** | Hematokrit centrifuge | heamatocrite with rotor for 24 capillaries | 1 |  |

Signed………………………………. Date…………………………... Stamp …………………………….

Name of Person Signing: ……………………………………………………………

Position in The Company: ………………………………………………………………

Company name: ………………………………………………………………………………………