# MINIMUM RECOMMENDED KIT / KIT SPECIFICATIONS

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **REF** | **ITEM**  | **Specification and description** | **Unit** | **Quantity** | **Unit Price** | **Total Price** |
| ***Plastic Sheeting/film LOT*** |
| 1 | Plastic sheeting heavy duty with at least 190g/m2 finished size of 4m width and 10 lm to 20 lm length per sheet | Material: made of woven high-density black polyethylene (HDPE) fibers.warp x weft, laminated on both sides with low-density polyethylene (LDPE) coating, with reinforced rims by heat sealing on all sides. Tensile strength: minimum 600 N in both directions of warp and weft. Tear strength: under ISO 4674 (A2). UV resistance: under ASTM G53/94 (UVB 313 nm peak). Welding: under ISO 1421 plus additional procedure. Reinforcement eyelets: provided with aluminum eyelets or equivalent on four sheet sides of the single sheets. Tensile strength of the eyelets:  Minimum 700N inside the eyelets as per ISO 1421 Flame retardant under CPA I84  | sqm | 1 |  |  |
| 2 | Flex sheet with 440 g/m2 of minimum 60 sqm surface area | Material: PVC coated sheet with weight of 440 grams per square meter Tensile strength: minimum 600 N in both directions of warp and weft. Tear strength: under ISO 4674 (A2). UV resistance: under ASTM G53/94 (UVB 313 nm peak). Reinforcement eyelets with 20mm diameter and placed every 50cm. around the PVC sheet Welding: under ISO 1421 plus additional procedure.Reinforcement eyelets: provided with aluminum eyelets or equivalent on four sheet sides of the single sheets.  | Pce | 1 |  |  |
| 3 |  Clear Plastic film  | Nylon transparent, 100-micron thickness, 4m x 5m  | Pce  | 1 |   |  |
| ***TIMBER LOT***  |
| 1  | Timber 80mmx80mmx 3m (Nominal dimension)  | Anti-Stain or Kiln-dried (KD), unfinished surface, ASTM grade 3 or European equivalent, maximum 18% humidity, +3mm to -1mm section dimension tolerance @ 18% humidity content. Timber to be certified from sustainable harvest according PEFC or FSC or similar international standards  | Pce  | 1 |  |  |
| 2  | Timber 100mmx50m mx4m (Nominal dimension)  | Anti-Stain or Kiln-dried (KD), unfinished surface, ASTM grade 3 or European equivalent, maximum 18% humidity, +3mm to -1mm section dimension tolerance @ 18% humidity content. Timber to be certified from sustainable harvest according PEFC or FSC or similar international standards  | Pce  | 1 |  |  |
| 3  | Timber 100mmx25m mx4m (Nominal dimension)  | Anti-Stain or Kiln-dried (KD), unfinished surface, ASTM grade 3 or European equivalent, maximum 18% humidity, +3mm to -1mm section dimension tolerance @ 18% humidity content. Timber to be certified from sustainable harvest according PEFC or FSC or similar international standards  | Pce  | 1 |  |  |
| 4  | Plywood sheet 8 mm  | **Canadian Douglas Fir, Finnish Spruce, or similar.** A minimum of three piles are laid so the grain runs in orthogonal directions.244mmx122mm dimensions | Pce  | 1 |  |  |
| 5  | Plywood sheet 4 mm  | **Canadian Douglas Fir, Finnish Spruce, or similar.** A minimumofthree piles are laid so the grain runs in orthogonal directions. 244mmx122mm dimensions | Pce  | 1 |   |   |
|  6 | XPE foiled face Insulation roll  | -Layer 1: Aluminum foil 12 mic -Layer 2: Cross-linked polyethylene foam - has fire retardant characteristic - thickness: 8mm - apparent density: 38kg/cbm - foam color: preferred white -Layer 3: PE "polyethylene" anti-flaming white film; 55 mics  Dimension: (1.20m width) x (length may vary 15ml or 20ml or 25ml)  | Roll of 24 sqm  |  1 |  |  |
| ***Ironmongery LOT***  |
| 1  | Timber screws  | Galvanized mild steel. 4mm shank diameter x 25 mm long. with flat bulge-head, compatible with 6mm wide blade screwdriver described. below, 400g boxes  | Box of 400g | 1 |  |   |
| 2  | Roofing Nails A  | Galvanized mild steel. 4mm shank diameter x 60 mm long. Domed head. Rubber washers included.  | kg  | 1 |  |  |
| 3  | Roofing Nails B  | Galvanized mild steel. 3mm shank diameter x 40 mm long. Domed head. Rubber washers included.  | kg  | 1 |  |  |
| 4  | Timber nails - 30mm  | Galvanized mild steel. 2mm shank diameter x 30mm length. With bulge-head  | kg  | 1 |  |  |
| 5  | Timber nails - 50mm  | Galvanized mild steel. 4mm shank diameter x 50mm length. With bulge-head  | kg  | 1 |  |  |
| 6  | Timber nails - 75mm  | Galvanized mild steel. 4mm shank diameter x 75mm length. With bulge-head  | kg  | 1 |  |  |
| 7  |  Steel angle sections  | Galvanized mild steel. Folded into a 90-degree angle. Minimum size = 10x10x2.5cm (i.e., each out-stand leg = 10cm long). Minimum plate thickness = 3mm. pre-drilled with a minimum of 3 holes per out-stand leg.  | Pce  | 1 |  |  |
| 8  | Rubber Ties  | Black, square section 15mm. Roll of 50 meters  | Pce  | 1 |  |  |
| 9  |  Stapler (with adequate staples)  | Staples Gun Tacker - Medium Duty - Manual To be provided with staples (1500 pcs): - Galvanized Steel wire - U Shapes - Stiff, flat wire (crown width: 12 - 13mm; Width: ~1mm to 1.2mm; Leg length: 12-13 mm; Thickness: 0.7-0.8 mm  | Pce  | 1 |  |  |
| 10  | Hinges  | Galvanized mild steel. T-shaped barrel hinge. Minimum 15cm long x 3cm wide outstanding arm. Minimum 7cm long x 3cm wide base plate. Predrilled with a minimum 4 no. of holes on each side of the hinge  | Pce  | 1 |  |  |
| 11  | Hasp  | Galvanized mild steel. Minimum 10cm length x 3cm wide. Minimum 4 no. pre-drilled holes per component for fixing. To be compatible with the padlock described below.  | Pce  | 1 |  |  |
| 12  | Padlock  | Galvanized mild steel. Body size minimum 4x4x2cm. Shackle minimum 6mm diameter. To be supplied with a minimum 2 no. keys  | Pce  | 1 |  |  |
| 13  | Flue Pipe  | Galvanized mild steel or stainless-steel tube. Minimum 15cm diameter x 50cm length. Preferably with minimum 50mm width out-stand flange (collar) welded to the exterior of the tube. | Pce  | 1 |  |  |
| 14 | Insulation adhesive tape  | Polyethylene reinforced Insulation Tape - High tacker - Roll of 6cm x 50m  | Pce  | 1 |  |  |
| ***Tool LOT*** |
| 1  | Carpentry Hammer  | Minimum overall length = 35cm long. Wooden or rubber-coated handle. Solid metal head with curved claws. Weight ~ 700 gr  | Pce  | 1 |  |  |
| 2  | Wood Saw  | Minimum overall length = 50cm long. Wooden or rubber-coated handle. Tapered  | Pce  | 1 |  |  |
| 3  | Cutter  | ("Stanley knife") - plastic or rubber handle - 2 pcs spare blades  | Pce  | 1 |  |  |
| 4  | Screwdriver  | 6mm wide blade-head, Shaft length: 12.5cm, Minimum overall length: 22cm.Wooden or rubber-coated handle. Fully insulated. Small mains tested:200-250 volts AC. Must fit woodscrews listed above  | Pce  | 1 |  |  |
| 5  | Tape Measure  | 10m length. Hand-coil (not sprung). Circular/disc shaped. Preferred metal case. | Pce  | 1 |  |  |