**Rolling Shutters Specifications**

**Item#SL005673**

**10.5 INTERNAL CURTAINS**

**GENERAL**

Furnish all labor, materials, tools, equipment, and services for internal curtains in accordance with provisions of Contract Documents.

**QUALITY ASSURANCE**

A. Source of Materials: Provide materials obtained from one source acceptable to Engineer for type and colour of internal curtains and setting materials.

**SUBMITTALS:**

A. Product data:

1. Manufacturer’s literature for internal curtains and installation materials.

2. Manufacturer’s instructions for installation.

B. Samples:

1. Samples of colors of internal curtains.

C. Project data:

1. Certification of applicator qualifications. The applicator should be qualified.

**EQUIPMENT**

A. ROLLER TUBE

The fabric rolls around the metal tube which supports the weight of the shade, is not to be exposed even when the shade is fully lowered.

B. END PLUG

The end plug or rotator to be fit into the installation bracket.

C. FABRIC

Design and colour to be approved by the Engineer.

NS/AM/L2019-02 - V2-Part-1 - Sec 10-05 2 of 2

D. BOTTOM OF CURTAIN

Add bottom rod and end cap to curtain to hold the fabric in position and add weight to the shade.

E. CLUTCH

Provide clutch to curtain to rotate the roller tube to raise or lower the shade.

F. CURTAIN CORD

Provide necessary cord items:

- Beaded cord for continuous loop.

- Beaded cord connector to attach the two ends of the beaded cord.

- Cord tensioner for enhanced child safety.