|  |  |
| --- | --- |
| **{HADATHA Association-****North Lebanon-Akkar-Berqael****Hadatha Bldg –f2}****[1/6/2023]****To:** **Request for Quotation No**. [HAD-CAR-RFQ-023-007/Solar Power in wadi Khaled center ]. | **] جمعية الحداثة - شمال لبنان / عكار-****برقايل -مبنى الحداثة –ط2[****1/6/2023****إلى:** [ ] **طلب اسعار رقم** HAD-CAR-RFQ-023-007**،تركيب طاقة شمسية في مركز وادي خالد ]** |
| **Dear Sir/Madam,**The Hadatha Association hereby request you to submit price quotation(s) for the supply of the item(s) listed on the attached Bidding Form titled ‘RFQ No**.** . [HAD-CAR-RFQ-023-007/ Solar Power in wadi Khaled center]. | **حضرة السيّدة /السيَد،** إنّ جمعية الحداثة تقدّم إليكم في ما يلي بطلب عرض / عروض اسعار لتوريد السّلعة/ السّلع المذكورة في نموذج العرض المرفق تحت عنوان" طلب اسعار رقم **[**HAD-CAR-RFQ-023-007 **تركيب طاقة شمسية في مركز وادي خالد ]** |
| You should submit one original of the attached Bidding Form. On the same form you also have to indicate your present stock and the delivery period. Your quotation should be sealed in an envelope, clearly marked ‘Quotation No. **[**HAD-CAR-RFQ-023-007**]** and delivered to the address above.  | يجب عليكم تقديم النسخة الاصلية من نموذج العرض المرفق. كما عليكم الاشارة في النموذج ذاته إلى مخزونكم الحالي وتاريخ التسليم. يجب أن يًقدّم عرضكم في ظرف مختوم ويُدوّن عليه بشكل واضح "عرض اسعار رقمHAD-CAR-RFQ-023-007ويُسلّم إلى العنوان المذكور اعلاه. |
| The deadline for receipt of your quotation is **[**4:00 **PM ]** on **[14/6/2023**]**,** at the address above.You quotation should be submitted as per the following instructions.  | الموعد النهائي لاستلام عرضكم هو **[الساعة الرابعة ظهرا ]** من **14-6-2023** على العنوان المذكور اعلاه. يجب أن يُقدّم العرض حسب التعليمات التاليّة:  |
| 1. **Prices:** The prices should be quoted for supply and delivery to **HADATHA destination Point as given in the attached Bidding Form**.
2. **Evaluations of Quotations:** Offers determined to be substantially responsive to the technical specifications will be evaluated by comparison of their prices
3. The delivery lead time will also be a consideration in the contract award.
4. **Award of Purchase Order:** The contract award will be made to the bidder offering the best value for money (lowest acceptable evaluated price). The successful bidder will sign a Contract (Purchase Order) as per the attached General Conditions of Contract for Procurement of Goods and must also sign and uphold the Hadatha Code of Ethics.
5. **Validity of the Offer**: Your quotation should be valid to 31st of December 2023
 | 1. **الاسعار**: تشمل الاسعار المعروضة توريد وتسليم البضاعة **إلى نقطة الاستلام المحدّدة في نموذج العرض المرفق.**
2. **تقييم عرض الاسعار:** إنّ العروض الّتي يتبيّن أنّها مطابقة إلى حدّ كبير للمواصفات الفنيّة يتمّ تقييمها بمقارنة اسعارها.
3. إنّ الوقت المحدّد للتسليم يؤخذ أيضاً بعين الاعتبار لمنح العقد.
4. **منح أمر الشّراء:** يُمنح العقد لمقدّم العرض الّذي يؤمن الجودة الافضل بالّسّعر الافضل (السّعر الادنى المقبول بالتقييم). يقوم مقدّم العرض المُختار بتوقيع العقد (طلب الشراء) حسب شروط الرابطة لعقد شراء السّلع المرفقة كما يجب أن يوقّع ويتمسّك بقواعد السّلوك الّتي يحدّدها جمعية الحداثة.

  **صلاحيّة العرض**: يبقى عرض الاسعار صالح لآخر كانون الاول2023 |
| All enquires and questions should be addressed to: **[Safa Karhani & Procurement officer /Hadatha-Berkael, 71-936804 :Safa.hadatha@outlook.com]**Under Hadatha’s Anticorruption Policy Bidders shall observe the highest standard of ethics during the procurement and execution of such contracts. HADATHA will reject a Bid if it determines that the Bidder recommended for award, has engaged in corrupt, fraudulent, collusive, or coercive practices in competing for, or in executing, the Contract. Yours sincerely | توجّه كافة الاستفسارات والاسئلة إلى : **[صفا قرحاني مسؤؤل مشتريات /جمعية الحداثة –برقايل /ه :****71-936804 :Safa.hadatha@outlook.com**بناءً على سياسة جمعية الحداثة في محاربة الفساد، يجب على مقدّمي العروض احترام أعلى معايير الاخلاقيّات خلال وضع العرض وتنفيذ العقد المرتبط به. وسترفض الرابطة العرض إذا تبيّن له أنّ مقدّم العرض المرشّح لمنح العقد متورّطٌ بعمليّات فساد أو اختلاس او تواطؤ أو ممارسات اكراهيّة في التنافس على هذا العقد او في تنفيذه. اليكم جزيل الاحترام  |

**HADATHA FORM – Request for Quotation No: \_\_\_** **HAD-CAR-RFQ-023-007\_\_\_\_**

**نموذج عرض طلب الاسعار الخاص بجمعية الحداثة– طلب عرض اسعار رقم: ... HAD-CAR-RFQ-023-007....**

|  |  |
| --- | --- |
| *HADATHA to complete خاص بجمعية الحداثة*  | *Bidder to complete خاص بمقدّم العرض*  |
| **Ser****رقم** | **Item Required****الغرض المطلوب** | **Specification****المواصفات** | **Quantity required****الكمية المطلوبة** | **Offered specification** **(if different from required)****المواصفات المعروضة (في حال اختلافها عمّا هو مطلوب)** | **Quantity offered****الكمية المعروضة** | **Unit price****سعر الوحدة** | **Total Price** **السعر الإجمالي** |
| **1** | Monocrystalline panels | Supply and Install of a PV array, including wiring (with earth connection) and accessoriesMinimum PV power: 545 Wp or equivalent to reach 3.5 KWP- Module Efficiency STC (%) at least 20.5%- Measures against Potential Induced Degradation on PV side and/or Inverter side.- Connectors to be certified- The system shall include:- All fixing accessories on module framing.- Earthing of the components- Device preventing any risk of an electrolytic couple- Reports of flash testing of the modules to be provided before installation.-Certifications requested: IEC 61215 – EN/IEC 61730 or similar, All certifications have to be issued by an internationally recognized laboratory.- Declaration letter from the manufacturer stating the date of manufacturing of the panels | **6** |  |  |  |  |
| **2** | Inverter | Supply and install of dual-mode 3.5 KW inverter, complete with configuration accessories and wiring | **1** |  |  |  |  |
| **3** | Batteries | Tubular, Lead-Acid Batteries CTT-200, for renewable energy storage to be used for the night critical load. Battery capacity = 200 Ah, battery nominal voltage = 12 V | **2** |  |  |  |  |
| **4** | Electric Work | Supply and Install Electrical Works and complete system connection including earthing of the systemPV generator wiring and associated components are exposed to UV, wind, water and other environmental conditions. Wiring and components should be fit for this purpose and built in such a way as to minimize exposure to detrimental environmental effects. Particular attention is drawn to the need for prevention of water accumulation in cable/module support systems.Preferably all accessories should be of European brand. The system should include the below items (the below list is not exhaustive, and items are not limited to the below)- Surge arrestors on DC and on AC (class B and C)- Cables are Cu/PVC/PVC (black) 600V/1000V Or Areal AL torsade typeBrands: Cables du Liban or similar- DC Cables and wiring should comply with the international standard EN 50618- H1Z2Z2-K, should DC solar power cable- Cable passages to be provided for DC cables, AC Cables and data cables for monitoring- All cables should be routed in cable trays- Junction Boxes for parallel connection of string cables and group cables (if any) for connecting modules to the inverter’s input. Class II boxes suitable for outdoor use (minimum IP65 protection) should be provided, it should include suitable DC fuses on each (+) and (-) polarities if appropriate.- Protective device against transient overvoltage, suitable for AC circuits (in accordance with EN 61643-11 or equivalent), type I or II according to justifications- All other accessories that deemed necessary to the good functioning and protection of the system | **1** |  |  |  |  |
| **5** | Steel structure | Steel structure made of galvanized hollow tube 60mmx30mm for columns and main beams, and40mmx40mm for secondary beams. Rates include panel installation using aluminum clamps, bolts, washers, and nuts. Each PV panel will be laid upon 3 hollow tubes (40x40mm). | **1** |  |  |  |  |
|  |  | **Supply & Installation of a Single-Phase PV System with a minimum total PV capacity****of 3.5 KWp** |  |  |  | **Total** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|   (تاريخ التسليم المطلوب) **Required Delivery Date:**  |  |  | (تاريخ التسليم المعروض)**Offered Delivery Date**: |  |
|  **(مكانالتسليم المطلوب)****Required Delivery Destination:** |  |  |  (مكان التسليم المعروض)**Offered Delivery Destination:** |  |
| (يبقى العرض صـــــالح لمدة)**This Bid is valid for:**  | \_\_days ((يوماً |  |  (بلد المنشأ للبضاعة المعروضة)**Country of Origin of offered Items:** |  |
| (اسم الشركة)**Company Name:** |  |  | (رقم الفاكس)**Facsimile No:**  |  |
| (العنوان)**Address:** |  |  | (رقم الهاتف)**Phone No:** |  |
|  |  |  | (البريد الالكتروني)**Email Address:** |  |

I certify that I have read and understood the Hadatha General Conditions of Contract for the Procurement of Goods and the Hadatha Code of Ethics. I further certify that the above-mentioned company has not engaged in corrupt, fraudulent, collusive, or coercive practices in competing for, or in executing, any Contracts.

أقر أنني قرأت وفهمت شروط الرابطة العامة لعقد مشتريات السّلع والقواعد السلوكية التي يحدّدها جمعية الحداثة. كذلك أقر أنّ الشركة المذكورة اعلاه غير متورّطة بأي ممارسات فساد أو اختلاس او تواطؤ أو ممارسات اكراهيّة في التنافس على هذا العقد او في تنفيذه.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| (الموقِّع)**Signed** | : |  |  | (المنصب)**Company Position** | : |  |
|  |  |  |  |  |  |  |
| (الإسم باحرف مطبوعة)**Print Name** | : |  |  | (التاريخ)**Date** | : |  |

*Please stamp this Bid Form with your Company Stamp*

*يرجى ختم المناقصة بختم الشركة الخاص بك*